### SECTION 216 – HORIZONTAL DIRECTIONAL DRILLING

**DESCRIPTION**

**METHOD OF MEASUREMENT**

**216.04.01 MEASUREMENT**

***ADD THE FOLLOWING TO THIS SUBSECTION:***

The quantity of XX INCH CONDUIT (DIRECTIONAL DRILL) will be measured per linear foot.

**METHOD OF PAYMENT**

**216.05.01 PAYMENT**

***ADD THE FOLLOWING TO THIS SUBSECTION:***

The accepted quantity of XX INCH CONDUIT (DIRECTIONAL DRILL) will be paid for at the contract unit price of linear foot and shall include all materials, equipment and labor required including, but not limited to, all piping and equipment required for the horizontal directional drilled installation of product pipe, complete and in place. Payment will also include all related excavation; shoring and bracing; compaction; post video of all sewer and storm facilities; restoration of damaged facilities; testing; disinfecting; and connections to existing lines or works and all other items necessary to complete the work as shown on the Plans, as specified herein and as directed by the Engineer.

Payment will be made under:

|  |  |  |
| --- | --- | --- |
| **ITEM NO.** | **ITEM DESCRIPTION** | **UOM** |
| 216.XXXX | XX INCH CONDUIT (DIRECTIONAL DRILL) | LF |

**END OF SECTION 216**