### SECTION 402 – PLANTMIX BITUMINOUS SURFACE

**METHOD OF MEASUREMENT**

**402.04.01 MEASUREMENT**

***delete this subsection in its entirety and replace with the following:***

The quantity of (X-INCH) PLANTMIX BITUMINOUS SURFACE will be measured per square yard.

**BASIS OF PAYMENT**

**402.05.01 PAYMENT**

***DELETE PARAGRAPH ”A” OF THIS SUBSECTION AND REPLACE WITH THE FOLLOWING:***

The accepted quantity of (X-INCH) PLANTMIX BITUMINOUS SURFACE will be paid for at the contract unit price of square yard and shall include all materials, equipment and labor required including, but not limited to, asphalt cement; mixing; loading; hauling; placing; compacting; tack coat; prime coat and all other items necessary to complete the work as shown on the Plans, as specified herein and as directed by the Engineer

Payment will be made under:

|  |  |  |
| --- | --- | --- |
| **ITEM NO.** | **ITEM DESCRIPTION** | **UOM** |
| 402.XXXX | (X-INCH) PLANTMIX BITUMINOUS SURFACE | SY |

**END OF SECTION 402**