### SECTION 403 – PLANTMIX BITUMINOUS OPEN-GRADED SURFACE

**MATERIALS**

**403.02.02 COMPOSITION OF MIXTURE**

***Add the following to this subsection:***

K. The grade of asphalt to be used for Plantmix Bituminous Open-graded surface shall be PG-76 as specified in Subsection 703.03.02.

**METHOD OF MEASUREMENT**

**403.04.01 MEASUREMENT**

***Add the following to this subsection:***

The quantity of 3/4-INCH PLANTMIX BITUMINOUS OPEN-GRADED SURFACE will be measured per square yard.

**BASIS OF PAYMENT**

**403.05.01 PAYMENT**

***Add the following TO this subsection:***

The accepted quantity of 3/4-INCH PLANTMIX BITUMINOUS OPEN-GRADED SURFACE will be paid for at the contract unit price of square yard and shall include all materials, equipment and labor required including, but not limited to, asphalt cement; mixing; loading; hauling; placing; compacting and all other items necessary to complete the work as shown on the Plans, as specified herein and as directed by the Engineer.

Payment will be made under:

|  |  |  |
| --- | --- | --- |
| **ITEM NO.** | **ITEM DESCRIPTION** | **UOM** |
| 403.0030 | 3/4-INCH PLANTMIX BITUMINOUS OPEN GRADED SURFACE | SY |

**END OF SECTION 403**