### SECTION 405 – TACK COAT

**MATERIAL**

**405.02.01 BITUMINOUS MATERIAL**

***DELETE PARAGRAPH “A.1” AND REPLACE WITH THE FOLLOWING:***

1. 1. The grade may be changed by the Engineer during construction and no additional compensation will be allowed.

**CONSTRUCTION**

**405.03.02 WEATHER LIMITATIONS**

***ADD THE FOLLOWING TO THIS SUBSECTION:***

B. Application of bituminous material shall be in accordance with subsection 401.03.05 "Weather Limitations".

**405.03.03 PREPARATION OF SURFACE**

***delete paragraph “a” of this subsection and replace with the following:***

A. The existing surface shall be patched and cleaned and be free of irregularities to provide a smooth and uniform surface to receive the treatment. The edges of existing pavements shall be sawcut to full depth, in a neat line and shall be cleaned prior to the application of a tack coat.

**405.03.04 APPLICATION OF ASPHALTIC EMULSION**

***DELETE PARAGRAPH “C.1” AND REPLACE WITH THE FOLLOWING:***

C. 1. Tack coat shall be applied to no greater area in any one day than is planned to be covered by plantmix during the same day.

**METHOD OF MEASUREMENT**

**405.04.01 MEASUREMENT**

***DELETE THIS SUBSECTION IN ITS ENTIRETY AND REPLACE WITH THE FOLLOWING:***

No direct measurement shall be made for Tack Coat.

**BASIS OF PAYMENT**

**405.05.01 PAYMENT**

***DELETE PARAGRAPHS “A”, “B” AND “E” OF THIS SUBSECTION AND ADD THE FOLLOWING PARAGRAPH:***

Unless otherwise provided in the Special Provisions, no payment will be made for Tack Coat as such. The cost thereof shall be considered as included in the price bid for construction or installation of the items to which Tack Coat is required.

**END OF SECTION 405**