### SECTION 413 – PLANTMIX BITUMINOUS GAP-GRADED SURFACE (UTACS)

**METHOD OF MEASUREMENT**

**413.04.01 MEASUREMENT**

***DELETE THIS SUBSECTION IN ITS ENTIRETY AND REPLACE WITH THE FOLLOWING:***

The quantity of UTACS BONDED WITH A PMM, S3 GRADATION (1-INCH) will be measured per square yard.

**BASIS OF PAYMENT**

**413.05.01 PAYMENT**

***Add the following TO this subsection:***

The accepted quantity of UTACS BONDED WITH A PMM, S3 GRADATION (1-INCH) will be paid for at the contract unit price of square yard and shall conform to the requirements of subsection 413.05.01 of the Uniform Standard Specifications and shall include all materials, equipment, labor and all work as shown on the Plans, as specified herein and as directed by the Engineer. The above payment includes demobilization or mobilization required to comply with application weather requirements of Subsection 413.03.06.

Payment will be made under:

|  |  |  |
| --- | --- | --- |
| **ITEM NO.** | **ITEM DESCRIPTION** | **UOM** |
| 413.0120 | UTACS BONDED WITH A PMM, S3 GRADATION (1.0 INCH) | SY |

**END OF SECTION 413**