### SECTION 505 – REINFORCING STEEL

**MATERIALS**

**505.02.01 GENERAL**

***add The following to this subsection:***

F. At selected locations as indicated on the Contract Drawings, reinforcing steel shall be galvanized (zinc coated), in accordance with ASTM A767 or epoxy-coated.

G. At the expansion joint locations shown on the Contract Drawings or as directed by the Engineer, reinforcing steel shall be sprayed, coating the entire circumference of the bar, with a zinc-rich formulation conforming to ASTM A767.

**METHOD OF MEASUREMENT**

**505.04.01 MEASUREMENT**

***delete this subsection in its entirety and replace with the following:***

No direct measurement shall be made for Reinforcing Steel.

**BASIS OF PAYMENT**

**505.05.01 PAYMENT**

***delete this subsection in its entirety and replace with the following:***

Unless otherwise provided in the Special Provisions, no payment will be made for Reinforcing Steel as such. The cost thereof shall be considered as included in the price bid for construction or installation of the items to which such Reinforcing Steel is required.

**END OF SECTION 505**