### SECTION 625 – CONSTRUCTION SIGNS

**MATERIALS**

**625.02.01 GENERAL**

***add The followiNG to this subsection:***

C. Reflective sheeting shall be used on all work zone signs and channelizing devices.

**CONSTRUCTION**

***Add The following SUBSECTIONS TO THIS SECTION:***

**625.03.05 PORTABLE CHANGEABLE MESSAGE SIGNS**

A. Portable Changeable Message Signs (PCMS) conforming to the MUTCD, Part 6, Section 6F.60 shall be used to advise the driver of road closures on streets with an 80-foot or greater right-of-way.

B. The PCMS shall be placed far enough in advance of the closed street to allow traffic ample opportunity to detour around the disrupted area.

C. The location and number of PCMS will be determined by the Engineer.

D. Solar powered panels shall be used in residential areas.

**625.03.06 ARROW DISPLAYS**

A. Arrow Displays conforming to the MUTCD, Part 6, Section 6F.61, Type B, shall be used to advise the driver of lane closures when so directed by the Engineer.

B. The Arrow Displays shall be required at the beginning of the taper and placed behind the barricades in the closed lanes, as required by the approved traffic control plan and as directed by the Engineer.

C. Solar powered panels shall be used in residential areas.

**METHOD OF MEASUREMENT**

**625.04.01 MEASUREMENT**

***Add The followinG TO THIS SUBSECTION:***

No direct measurement shall be made for PORTABLE CHANGEABLE MESSAGE SIGN or ARROW DISPLAY.

**BASIS OF PAYMENT**

**625.05.01 PAYMENT**

***Add The followinG TO THIS SUBSECTION:***

Unless otherwise provided in the Special Provisions, no payment will be made for PORTABLE CHANGEABLE MESSAGE SIGN or ARROW DISPLAY as such. The cost thereof shall be considered as included in the price bid for TRAFFIC CONTROL AND MAINTENANCE.

**END OF SECTION 625**