### SECTION 616 – FENCING

**DESCRIPTION**

**616.01.01 GENERAL**

***ADD THE FOLLOWING PARAGRAPHS TO THIS SUBSECTION:***

D. Temporary fencing will be required in association with chain link fence installation to maintain the integrity of fencing around private properties until the new fencing is complete. Temporary fencing shall be considered incidental to the chain link fence item and no additional compensation will be allowed. Temporary fencing is to meet the requirements of this subsection and shall be installed prior to the removal of existing fencing and shall remain in place until the new fence is complete.

**MATERIALS**

**616.02.01 GENERAL**

***ADD THE FOLLOWING PARAGRAPHS TO THIS SUBSECTION:***

B. Include one Masterlock 178D lock and 2’ long section of Blue Hawk heavy duty grade 70 4,700 tow pound chain for each gate installed.

**METHOD OF MEASUREMENT**

**616.04.01 MEASUREMENT**

***ADD THE FOLLOWING PARAGRAPHS TO THIS SUBSECTION:***

The quantity of XX-FOOT CHAIN LINK FENCE will be measured per linear foot.

The quantity of XX-FOOT SINGLE SWING CHAIN LINK GATE and XX-FOOT DOUBLE SWING CHAIN LINK GATE will be measured per each.

The quantity of [FILL IN ITEM DESCRIPTION] will be measured per [UNIT].

No direct measurement shall be made for [FILL IN ITEM DESCRIPTION].

**BASIS OF PAYMENT**

**616.05.01 PAYMENT**

***ADD THE FOLLOWING PARAGRAPHS TO THIS SUBSECTION:***

The accepted quantity of XX-FOOT CHAIN LINK FENCE will be paid for at the contract unit price of linear foot and shall include all labor, equipment and materials including but not limited to excavation; aggregate base materials; pipe; welding; backfill; compaction; connection to existing fencing; installation of temporary fencing until proposed fencing is installed and all other items necessary to complete the work as shown on the Plans, as specified herein and as directed by the Engineer.

The accepted quantity of XX-FOOT SINGLE SWING CHAIN LINK GATE and XX-FOOT DOUBLE SWING CHAIN LINK GATE will be paid for at the contract unit price of each and shall include all labor, equipment and materials including but not limited to excavation; aggregate base materials; pipe; welding; locks; chain; backfill; compaction; connection to existing fencing; installation of temporary gates until proposed gate is installed and all other items necessary to complete the work as shown on the Plans, as specified herein and as directed by the Engineer.

The accepted quantity of [FILL IN ITEM DESCRIPTION] will be paid for at the contract unit price of [UNIT] and shall include all materials, equipment and labor required including, but not limited to, [FILL IN] and all other items necessary to complete the work as shown on the Plans, as specified herein and as directed by the Engineer.

The accepted quantity of [FILL IN ITEM DESCRIPTION] will be paid for at the contract unit price of [UNIT] and shall conform to the requirements of subsection 614.05.01 of the Uniform Standard Specifications and shall include all materials, equipment, labor and disposal required to perform this work and all work as shown on the Plans, as specified herein and as directed by the Engineer. The above payment shall also include,

Unless otherwise provided in the Special Provisions, no payment will be made for [FILL IN ITEM DESCRIPTION] as such. The cost thereof shall be considered as included in the price bid for construction or installation of the items to which [FILL IN ITEM DESCRIPTION] is required.

Payment will be made under:

|  |  |  |
| --- | --- | --- |
| **ITEM NO.** | **ITEM DESCRIPTION** | **UOM** |
| 616.XXXX | XX-FOOT CHAIN LINK FENCE | LF |
| 616.XXXX | XX-FOOT SINGLE SWING CHAIN LINK GATE | EA |
| 616.XXXX | XX-FOOT DOUBLE SWING CHAIN LINK GATE | EA |

**END OF SECTION 616**