### SECTION 627 – PERMANENT SIGNS

**DESCRIPTION**

**627.01.01 GENERAL**

***ADD THE FOLLOWING TO THIS SUBSECTION:***

E. The work shall include all labor, material, equipment and incidental hardware necessary to remove, relocate and/or install roadway street signs and posts.

F. The unit price shall include delivery of salvaged and unused signs to the City Maintenance Yard located at 3100 East Bonanza Avenue, Building A. The Contractor must call (702) 229-6331, 24-hours in advance of delivery. The Contractor must also have the ability to unload their truck without use of City facilities or equipment.

**MATERIALS**

**627.02.01 GENERAL**

***ADD THE FOLLOWING TO THIS SUBSECTION:***

B. All new permanent signs shall utilize Type XI retroreflective sheeting in accordance with USS sections 627 and 716 and shall have an anti-graffiti protective overlay film that is a matching component to, and of the same manufacturer as the retroreflective sheeting to which it is applied.

**CONSTRUCTION**

**627.03.03 INSTALLATION**

***ADD THE FOLLOWING TO THIS SUBSECTION:***

K. Directional signs that are not functional may require covering during the progress of the work.

1. Covers shall be sufficient size and density to completely block out the message so that it is not visible either during the day or night.
2. The use of burlap or similar fabrics will not be allowed.
3. Covers shall be fastened securely to prevent movement by wind action and withstand the effect of weathering.
4. No adhesive tape shall be applied to the face of the sign.

**METHOD OF MEASUREMENT**

**627.04.01 MEASUREMENT**

***ADD THE FOLLOWING TO THIS SUBSECTION:***

The quantity of INSTALL NEW SIGN (GROUND MOUNTED) will be measured per each.

The quantity of [FILL IN ITEM DESCRIPTION] will be measured per [UNIT].

No direct measurement shall be made for [FILL IN ITEM DESCRIPTION].

**BASIS OF PAYMENT**

**627.05.01 PAYMENT**

***ADD THE FOLLOWING TO THIS SUBSECTION:***

The accepted quantity of INSTALL NEW SIGN (GROUND MOUNTED) will be paid for at the contract unit price of each and shall include all materials, equipment and labor required to fabricate and install the signs including, but not limited to, excavation; backfill; concrete foundation; supports; poles; hardware; making all required tests and all other items necessary to complete the work as shown on the Plans, as specified herein and as directed by the Engineer.

The accepted quantity of [FILL IN ITEM DESCRIPTION] will be paid for at the contract unit price of [UNIT] and shall include all materials, equipment and labor required including, but not limited to, [FILL IN] and all other items necessary to complete the work as shown on the Plans, as specified herein and as directed by the Engineer.

The accepted quantity of [FILL IN ITEM DESCRIPTION] will be paid for at the contract unit price of [UNIT] and shall conform to the requirements of subsection 627.05.01 of the Uniform Standard Specifications and shall include all materials, equipment, labor and disposal required to perform this work and all work as shown on the Plans, as specified herein and as directed by the Engineer. The above payment shall also include,

Unless otherwise provided in the Special Provisions, no payment will be made for [FILL IN ITEM DESCRIPTION] as such. The cost thereof shall be considered as included in the price bid for construction or installation of the items to which [FILL IN ITEM DESCRIPTION] is required.

All payments will be made in accordance with Subsection 109.02, “Scope of Payment”.

Payment will be made under:

|  |  |  |
| --- | --- | --- |
| **ITEM NO.** | **ITEM DESCRIPTION** | **UOM** |
| 627.0190 | INSTALL NEW SIGN (GROUND MOUNTED) | EA |

**END OF SECTION 627**